

DSEAR Zone 2- Explosive atmosphere may occur under abnormal operation and only persists for a short period.

ATEX Category 3 - Equipment must be safe under normal operation.