

Basement to the pump motor housing is categorised by way of the National Categories and City & Guilds 6150 Scheme as:

**NC3 When not possible to have continuous attachment to a safety line. Typically where the work team must move away from the point of entry.**